|  | Configuring the NetSpot Device Installer for TCP/IP environment

| Setting and Referencing the Device Information Acquisition Interval

This section describes the procedure for setting the device search interval and the update interval for the device status that is displayed in the device list on the main screen. The interval set here is used when automatically updating the device status or searching for devices.

1. Select [Polling Intervals] from the [Options] menu.
2. Reference or set the device status update interval and the device search interval in the [Polling Interval Settings] dialog box.

   [Get Device Status Every]:
     Select the interval for updating device status that is displayed in the device list update interval.
   [Discover Device Every]:
     Select the search interval for devices.

   | If [Not Specified] is selected for [Get Device Status Every], you can only select [Not Specified] for [Discover Device Every].

3. Click the [OK] button after configuring all the items.

   | The settings are now enabled.