|  | Configuring the NetSpot Device Installer for TCP/IP environment

| Setting and Referencing the IP Address Pool

This section describes how to set up and display the IP address pool.

| By specifying a range of IP addresses for the IP address pool, you can make settings so that an unused IP address is automatically assigned from the IP address pool when configuring an IP address settings for the first time. To set an IP address for each device using the IP address pool, refer to Setting Only an IP Address (Easy Setup).
To set IP addresses for a number of devices using the IP address pool, refer to Batch Settings for Multiple Devices.

1. Select [IP Address Pool] from the [Options] menu.
2. Reference and set up the IP address pool in the [IP Address Pool Settings] dialog box.

   [IP Address]:
     IP address in the IP address pool.
   [MAC Address]:
     MAC address of the device using the IP address.
   [Status]:
     Status of the IP address.

   | Follow the procedure described below in order to add IP addresses. Input the start of the range of IP addresses to be added in [First Address] and the end of the range in [Last Address], and then click the [Add] button. To add individual IP addresses, input only [First Address] and then click the [Add] button.
   | Follow the procedure described below in order to delete IP addresses. Select the IP addresses to be deleted from the IP address list, and then click the [Remove] button. (More than one IP address may be selected.)

3. Click the [OK] button after configuring all the items.

   | The settings are now enabled.