|  | Troubleshooting

| Cannot Confirm a Device with NetSpot Device Installer for IPX

Cause 1: | The power to the device is not turned on.
Action: | Turn the device's power on.
Cause 2: | The network board is not properly connected.
Action: | Turn the device's power off, confirm the following, and then turn the device's power back on.

| Refer to the network board manual, and confirm that the network board is installed correctly. (This operation is not necessary when using a device that offers standard support for network functions.)
| Refer to the network board manual and confirm that the device is connected to the network using the correct cable.
| If you are using 10Base-2, make sure that the network terminators are properly connected.

Cause 3: | The device's frame type is not correctly set.
Action: | Set a frame type that suits your system. You can make the setting with NetSpot Device Installer for TCP/IP.
|  |  |  |